[
  {
    "added_include_path": "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/cores/esp32"
  },
  {
    "added_include_path": "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/variants/esp32s3"
  },
  {
    "compile": {
      "source_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/sketch/voice_assistant.ino.cpp",
      "object_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/sketch/voice_assistant.ino.cpp.o",
      "depfile_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/sketch/voice_assistant.ino.cpp.d"
    },
    "compile_task": {
      "args": [
        "/home/sam/.arduino15/packages/esp32/tools/esp-x32/2411/bin/xtensa-esp32s3-elf-g++",
        "-c",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/cpp_flags",
        "-w",
        "-Os",
        "-Werror=return-type",
        "-w",
        "-x",
        "c++",
        "-E",
        "-CC",
        "-DF_CPU=240000000L",
        "-DARDUINO=10607",
        "-DARDUINO_ESP32S3_DEV",
        "-DARDUINO_ARCH_ESP32",
        "-DARDUINO_BOARD=\"ESP32S3_DEV\"",
        "-DARDUINO_VARIANT=\"esp32s3\"",
        "-DARDUINO_PARTITION_default",
        "-DARDUINO_HOST_OS=\"linux\"",
        "-DARDUINO_FQBN=\"esp32:esp32:esp32s3:CDCOnBoot=cdc,USBMode=hwcdc,PSRAM=disabled,FlashMode=dio,DebugLevel=info\"",
        "-DESP32=ESP32",
        "-DCORE_DEBUG_LEVEL=3",
        "-DARDUINO_RUNNING_CORE=1",
        "-DARDUINO_EVENT_RUNNING_CORE=1",
        "-DARDUINO_USB_MODE=1",
        "-DARDUINO_USB_CDC_ON_BOOT=1",
        "-DARDUINO_USB_MSC_ON_BOOT=0",
        "-DARDUINO_USB_DFU_ON_BOOT=0",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/defines",
        "-I/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant",
        "-iprefix",
        "/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/include/",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/includes",
        "-I/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/dio_qspi/include",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/cores/esp32",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/variants/esp32s3",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/build_opt.h",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/file_opts",
        "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/sketch/voice_assistant.ino.cpp",
        "-o",
        "/dev/null"
      ]
    }
  },
  {
    "missing_include_h": "WiFi.h"
  },
  {
    "added_include_path": "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src"
  },
  {
    "compile": {
      "source_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/sketch/voice_assistant.ino.cpp",
      "object_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/sketch/voice_assistant.ino.cpp.o",
      "depfile_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/sketch/voice_assistant.ino.cpp.d"
    },
    "compile_task": {
      "args": [
        "/home/sam/.arduino15/packages/esp32/tools/esp-x32/2411/bin/xtensa-esp32s3-elf-g++",
        "-c",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/cpp_flags",
        "-w",
        "-Os",
        "-Werror=return-type",
        "-w",
        "-x",
        "c++",
        "-E",
        "-CC",
        "-DF_CPU=240000000L",
        "-DARDUINO=10607",
        "-DARDUINO_ESP32S3_DEV",
        "-DARDUINO_ARCH_ESP32",
        "-DARDUINO_BOARD=\"ESP32S3_DEV\"",
        "-DARDUINO_VARIANT=\"esp32s3\"",
        "-DARDUINO_PARTITION_default",
        "-DARDUINO_HOST_OS=\"linux\"",
        "-DARDUINO_FQBN=\"esp32:esp32:esp32s3:CDCOnBoot=cdc,USBMode=hwcdc,PSRAM=disabled,FlashMode=dio,DebugLevel=info\"",
        "-DESP32=ESP32",
        "-DCORE_DEBUG_LEVEL=3",
        "-DARDUINO_RUNNING_CORE=1",
        "-DARDUINO_EVENT_RUNNING_CORE=1",
        "-DARDUINO_USB_MODE=1",
        "-DARDUINO_USB_CDC_ON_BOOT=1",
        "-DARDUINO_USB_MSC_ON_BOOT=0",
        "-DARDUINO_USB_DFU_ON_BOOT=0",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/defines",
        "-I/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant",
        "-iprefix",
        "/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/include/",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/includes",
        "-I/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/dio_qspi/include",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/cores/esp32",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/variants/esp32s3",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/build_opt.h",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/file_opts",
        "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/sketch/voice_assistant.ino.cpp",
        "-o",
        "/dev/null"
      ]
    }
  },
  {
    "missing_include_h": "Network.h"
  },
  {
    "added_include_path": "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src"
  },
  {
    "compile": {
      "source_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/sketch/voice_assistant.ino.cpp",
      "object_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/sketch/voice_assistant.ino.cpp.o",
      "depfile_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/sketch/voice_assistant.ino.cpp.d"
    },
    "compile_task": {
      "args": [
        "/home/sam/.arduino15/packages/esp32/tools/esp-x32/2411/bin/xtensa-esp32s3-elf-g++",
        "-c",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/cpp_flags",
        "-w",
        "-Os",
        "-Werror=return-type",
        "-w",
        "-x",
        "c++",
        "-E",
        "-CC",
        "-DF_CPU=240000000L",
        "-DARDUINO=10607",
        "-DARDUINO_ESP32S3_DEV",
        "-DARDUINO_ARCH_ESP32",
        "-DARDUINO_BOARD=\"ESP32S3_DEV\"",
        "-DARDUINO_VARIANT=\"esp32s3\"",
        "-DARDUINO_PARTITION_default",
        "-DARDUINO_HOST_OS=\"linux\"",
        "-DARDUINO_FQBN=\"esp32:esp32:esp32s3:CDCOnBoot=cdc,USBMode=hwcdc,PSRAM=disabled,FlashMode=dio,DebugLevel=info\"",
        "-DESP32=ESP32",
        "-DCORE_DEBUG_LEVEL=3",
        "-DARDUINO_RUNNING_CORE=1",
        "-DARDUINO_EVENT_RUNNING_CORE=1",
        "-DARDUINO_USB_MODE=1",
        "-DARDUINO_USB_CDC_ON_BOOT=1",
        "-DARDUINO_USB_MSC_ON_BOOT=0",
        "-DARDUINO_USB_DFU_ON_BOOT=0",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/defines",
        "-I/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant",
        "-iprefix",
        "/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/include/",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/includes",
        "-I/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/dio_qspi/include",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/cores/esp32",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/variants/esp32s3",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/build_opt.h",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/file_opts",
        "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/sketch/voice_assistant.ino.cpp",
        "-o",
        "/dev/null"
      ]
    }
  },
  {
    "missing_include_h": "PubSubClient.h"
  },
  {
    "added_include_path": "/home/sam/Arduino/libraries/PubSubClient/src"
  },
  {
    "compile": {
      "source_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/sketch/voice_assistant.ino.cpp",
      "object_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/sketch/voice_assistant.ino.cpp.o",
      "depfile_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/sketch/voice_assistant.ino.cpp.d"
    },
    "compile_task": {
      "args": [
        "/home/sam/.arduino15/packages/esp32/tools/esp-x32/2411/bin/xtensa-esp32s3-elf-g++",
        "-c",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/cpp_flags",
        "-w",
        "-Os",
        "-Werror=return-type",
        "-w",
        "-x",
        "c++",
        "-E",
        "-CC",
        "-DF_CPU=240000000L",
        "-DARDUINO=10607",
        "-DARDUINO_ESP32S3_DEV",
        "-DARDUINO_ARCH_ESP32",
        "-DARDUINO_BOARD=\"ESP32S3_DEV\"",
        "-DARDUINO_VARIANT=\"esp32s3\"",
        "-DARDUINO_PARTITION_default",
        "-DARDUINO_HOST_OS=\"linux\"",
        "-DARDUINO_FQBN=\"esp32:esp32:esp32s3:CDCOnBoot=cdc,USBMode=hwcdc,PSRAM=disabled,FlashMode=dio,DebugLevel=info\"",
        "-DESP32=ESP32",
        "-DCORE_DEBUG_LEVEL=3",
        "-DARDUINO_RUNNING_CORE=1",
        "-DARDUINO_EVENT_RUNNING_CORE=1",
        "-DARDUINO_USB_MODE=1",
        "-DARDUINO_USB_CDC_ON_BOOT=1",
        "-DARDUINO_USB_MSC_ON_BOOT=0",
        "-DARDUINO_USB_DFU_ON_BOOT=0",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/defines",
        "-I/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant",
        "-iprefix",
        "/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/include/",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/includes",
        "-I/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/dio_qspi/include",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/cores/esp32",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/variants/esp32s3",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src",
        "-I/home/sam/Arduino/libraries/PubSubClient/src",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/build_opt.h",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/file_opts",
        "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/sketch/voice_assistant.ino.cpp",
        "-o",
        "/dev/null"
      ]
    }
  },
  {
    "missing_include_h": "Freenove_WS2812_Lib_for_ESP32.h"
  },
  {
    "added_include_path": "/home/sam/Arduino/libraries/Freenove_WS2812_Lib_for_ESP32/src"
  },
  {
    "compile": {
      "source_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/sketch/voice_assistant.ino.cpp",
      "object_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/sketch/voice_assistant.ino.cpp.o",
      "depfile_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/sketch/voice_assistant.ino.cpp.d"
    },
    "compile_task": {
      "args": [
        "/home/sam/.arduino15/packages/esp32/tools/esp-x32/2411/bin/xtensa-esp32s3-elf-g++",
        "-c",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/cpp_flags",
        "-w",
        "-Os",
        "-Werror=return-type",
        "-w",
        "-x",
        "c++",
        "-E",
        "-CC",
        "-DF_CPU=240000000L",
        "-DARDUINO=10607",
        "-DARDUINO_ESP32S3_DEV",
        "-DARDUINO_ARCH_ESP32",
        "-DARDUINO_BOARD=\"ESP32S3_DEV\"",
        "-DARDUINO_VARIANT=\"esp32s3\"",
        "-DARDUINO_PARTITION_default",
        "-DARDUINO_HOST_OS=\"linux\"",
        "-DARDUINO_FQBN=\"esp32:esp32:esp32s3:CDCOnBoot=cdc,USBMode=hwcdc,PSRAM=disabled,FlashMode=dio,DebugLevel=info\"",
        "-DESP32=ESP32",
        "-DCORE_DEBUG_LEVEL=3",
        "-DARDUINO_RUNNING_CORE=1",
        "-DARDUINO_EVENT_RUNNING_CORE=1",
        "-DARDUINO_USB_MODE=1",
        "-DARDUINO_USB_CDC_ON_BOOT=1",
        "-DARDUINO_USB_MSC_ON_BOOT=0",
        "-DARDUINO_USB_DFU_ON_BOOT=0",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/defines",
        "-I/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant",
        "-iprefix",
        "/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/include/",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/includes",
        "-I/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/dio_qspi/include",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/cores/esp32",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/variants/esp32s3",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src",
        "-I/home/sam/Arduino/libraries/PubSubClient/src",
        "-I/home/sam/Arduino/libraries/Freenove_WS2812_Lib_for_ESP32/src",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/build_opt.h",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/file_opts",
        "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/sketch/voice_assistant.ino.cpp",
        "-o",
        "/dev/null"
      ]
    }
  },
  {
    "missing_include_h": ""
  },
  {
    "compile": {
      "source_path": "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src/AP.cpp",
      "object_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/WiFi/AP.cpp.o",
      "depfile_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/WiFi/AP.cpp.d"
    },
    "compile_task": {
      "args": [
        "/home/sam/.arduino15/packages/esp32/tools/esp-x32/2411/bin/xtensa-esp32s3-elf-g++",
        "-c",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/cpp_flags",
        "-w",
        "-Os",
        "-Werror=return-type",
        "-w",
        "-x",
        "c++",
        "-E",
        "-CC",
        "-DF_CPU=240000000L",
        "-DARDUINO=10607",
        "-DARDUINO_ESP32S3_DEV",
        "-DARDUINO_ARCH_ESP32",
        "-DARDUINO_BOARD=\"ESP32S3_DEV\"",
        "-DARDUINO_VARIANT=\"esp32s3\"",
        "-DARDUINO_PARTITION_default",
        "-DARDUINO_HOST_OS=\"linux\"",
        "-DARDUINO_FQBN=\"esp32:esp32:esp32s3:CDCOnBoot=cdc,USBMode=hwcdc,PSRAM=disabled,FlashMode=dio,DebugLevel=info\"",
        "-DESP32=ESP32",
        "-DCORE_DEBUG_LEVEL=3",
        "-DARDUINO_RUNNING_CORE=1",
        "-DARDUINO_EVENT_RUNNING_CORE=1",
        "-DARDUINO_USB_MODE=1",
        "-DARDUINO_USB_CDC_ON_BOOT=1",
        "-DARDUINO_USB_MSC_ON_BOOT=0",
        "-DARDUINO_USB_DFU_ON_BOOT=0",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/defines",
        "-I/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant",
        "-iprefix",
        "/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/include/",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/includes",
        "-I/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/dio_qspi/include",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/cores/esp32",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/variants/esp32s3",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src",
        "-I/home/sam/Arduino/libraries/PubSubClient/src",
        "-I/home/sam/Arduino/libraries/Freenove_WS2812_Lib_for_ESP32/src",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/build_opt.h",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/file_opts",
        "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src/AP.cpp",
        "-o",
        "/dev/null"
      ]
    }
  },
  {
    "missing_include_h": ""
  },
  {
    "compile": {
      "source_path": "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src/STA.cpp",
      "object_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/WiFi/STA.cpp.o",
      "depfile_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/WiFi/STA.cpp.d"
    },
    "compile_task": {
      "args": [
        "/home/sam/.arduino15/packages/esp32/tools/esp-x32/2411/bin/xtensa-esp32s3-elf-g++",
        "-c",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/cpp_flags",
        "-w",
        "-Os",
        "-Werror=return-type",
        "-w",
        "-x",
        "c++",
        "-E",
        "-CC",
        "-DF_CPU=240000000L",
        "-DARDUINO=10607",
        "-DARDUINO_ESP32S3_DEV",
        "-DARDUINO_ARCH_ESP32",
        "-DARDUINO_BOARD=\"ESP32S3_DEV\"",
        "-DARDUINO_VARIANT=\"esp32s3\"",
        "-DARDUINO_PARTITION_default",
        "-DARDUINO_HOST_OS=\"linux\"",
        "-DARDUINO_FQBN=\"esp32:esp32:esp32s3:CDCOnBoot=cdc,USBMode=hwcdc,PSRAM=disabled,FlashMode=dio,DebugLevel=info\"",
        "-DESP32=ESP32",
        "-DCORE_DEBUG_LEVEL=3",
        "-DARDUINO_RUNNING_CORE=1",
        "-DARDUINO_EVENT_RUNNING_CORE=1",
        "-DARDUINO_USB_MODE=1",
        "-DARDUINO_USB_CDC_ON_BOOT=1",
        "-DARDUINO_USB_MSC_ON_BOOT=0",
        "-DARDUINO_USB_DFU_ON_BOOT=0",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/defines",
        "-I/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant",
        "-iprefix",
        "/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/include/",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/includes",
        "-I/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/dio_qspi/include",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/cores/esp32",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/variants/esp32s3",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src",
        "-I/home/sam/Arduino/libraries/PubSubClient/src",
        "-I/home/sam/Arduino/libraries/Freenove_WS2812_Lib_for_ESP32/src",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/build_opt.h",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/file_opts",
        "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src/STA.cpp",
        "-o",
        "/dev/null"
      ]
    }
  },
  {
    "missing_include_h": ""
  },
  {
    "compile": {
      "source_path": "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src/WiFi.cpp",
      "object_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/WiFi/WiFi.cpp.o",
      "depfile_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/WiFi/WiFi.cpp.d"
    },
    "compile_task": {
      "args": [
        "/home/sam/.arduino15/packages/esp32/tools/esp-x32/2411/bin/xtensa-esp32s3-elf-g++",
        "-c",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/cpp_flags",
        "-w",
        "-Os",
        "-Werror=return-type",
        "-w",
        "-x",
        "c++",
        "-E",
        "-CC",
        "-DF_CPU=240000000L",
        "-DARDUINO=10607",
        "-DARDUINO_ESP32S3_DEV",
        "-DARDUINO_ARCH_ESP32",
        "-DARDUINO_BOARD=\"ESP32S3_DEV\"",
        "-DARDUINO_VARIANT=\"esp32s3\"",
        "-DARDUINO_PARTITION_default",
        "-DARDUINO_HOST_OS=\"linux\"",
        "-DARDUINO_FQBN=\"esp32:esp32:esp32s3:CDCOnBoot=cdc,USBMode=hwcdc,PSRAM=disabled,FlashMode=dio,DebugLevel=info\"",
        "-DESP32=ESP32",
        "-DCORE_DEBUG_LEVEL=3",
        "-DARDUINO_RUNNING_CORE=1",
        "-DARDUINO_EVENT_RUNNING_CORE=1",
        "-DARDUINO_USB_MODE=1",
        "-DARDUINO_USB_CDC_ON_BOOT=1",
        "-DARDUINO_USB_MSC_ON_BOOT=0",
        "-DARDUINO_USB_DFU_ON_BOOT=0",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/defines",
        "-I/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant",
        "-iprefix",
        "/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/include/",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/includes",
        "-I/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/dio_qspi/include",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/cores/esp32",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/variants/esp32s3",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src",
        "-I/home/sam/Arduino/libraries/PubSubClient/src",
        "-I/home/sam/Arduino/libraries/Freenove_WS2812_Lib_for_ESP32/src",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/build_opt.h",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/file_opts",
        "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src/WiFi.cpp",
        "-o",
        "/dev/null"
      ]
    }
  },
  {
    "missing_include_h": ""
  },
  {
    "compile": {
      "source_path": "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src/WiFiAP.cpp",
      "object_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/WiFi/WiFiAP.cpp.o",
      "depfile_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/WiFi/WiFiAP.cpp.d"
    },
    "compile_task": {
      "args": [
        "/home/sam/.arduino15/packages/esp32/tools/esp-x32/2411/bin/xtensa-esp32s3-elf-g++",
        "-c",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/cpp_flags",
        "-w",
        "-Os",
        "-Werror=return-type",
        "-w",
        "-x",
        "c++",
        "-E",
        "-CC",
        "-DF_CPU=240000000L",
        "-DARDUINO=10607",
        "-DARDUINO_ESP32S3_DEV",
        "-DARDUINO_ARCH_ESP32",
        "-DARDUINO_BOARD=\"ESP32S3_DEV\"",
        "-DARDUINO_VARIANT=\"esp32s3\"",
        "-DARDUINO_PARTITION_default",
        "-DARDUINO_HOST_OS=\"linux\"",
        "-DARDUINO_FQBN=\"esp32:esp32:esp32s3:CDCOnBoot=cdc,USBMode=hwcdc,PSRAM=disabled,FlashMode=dio,DebugLevel=info\"",
        "-DESP32=ESP32",
        "-DCORE_DEBUG_LEVEL=3",
        "-DARDUINO_RUNNING_CORE=1",
        "-DARDUINO_EVENT_RUNNING_CORE=1",
        "-DARDUINO_USB_MODE=1",
        "-DARDUINO_USB_CDC_ON_BOOT=1",
        "-DARDUINO_USB_MSC_ON_BOOT=0",
        "-DARDUINO_USB_DFU_ON_BOOT=0",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/defines",
        "-I/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant",
        "-iprefix",
        "/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/include/",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/includes",
        "-I/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/dio_qspi/include",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/cores/esp32",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/variants/esp32s3",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src",
        "-I/home/sam/Arduino/libraries/PubSubClient/src",
        "-I/home/sam/Arduino/libraries/Freenove_WS2812_Lib_for_ESP32/src",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/build_opt.h",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/file_opts",
        "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src/WiFiAP.cpp",
        "-o",
        "/dev/null"
      ]
    }
  },
  {
    "missing_include_h": ""
  },
  {
    "compile": {
      "source_path": "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src/WiFiGeneric.cpp",
      "object_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/WiFi/WiFiGeneric.cpp.o",
      "depfile_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/WiFi/WiFiGeneric.cpp.d"
    },
    "compile_task": {
      "args": [
        "/home/sam/.arduino15/packages/esp32/tools/esp-x32/2411/bin/xtensa-esp32s3-elf-g++",
        "-c",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/cpp_flags",
        "-w",
        "-Os",
        "-Werror=return-type",
        "-w",
        "-x",
        "c++",
        "-E",
        "-CC",
        "-DF_CPU=240000000L",
        "-DARDUINO=10607",
        "-DARDUINO_ESP32S3_DEV",
        "-DARDUINO_ARCH_ESP32",
        "-DARDUINO_BOARD=\"ESP32S3_DEV\"",
        "-DARDUINO_VARIANT=\"esp32s3\"",
        "-DARDUINO_PARTITION_default",
        "-DARDUINO_HOST_OS=\"linux\"",
        "-DARDUINO_FQBN=\"esp32:esp32:esp32s3:CDCOnBoot=cdc,USBMode=hwcdc,PSRAM=disabled,FlashMode=dio,DebugLevel=info\"",
        "-DESP32=ESP32",
        "-DCORE_DEBUG_LEVEL=3",
        "-DARDUINO_RUNNING_CORE=1",
        "-DARDUINO_EVENT_RUNNING_CORE=1",
        "-DARDUINO_USB_MODE=1",
        "-DARDUINO_USB_CDC_ON_BOOT=1",
        "-DARDUINO_USB_MSC_ON_BOOT=0",
        "-DARDUINO_USB_DFU_ON_BOOT=0",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/defines",
        "-I/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant",
        "-iprefix",
        "/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/include/",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/includes",
        "-I/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/dio_qspi/include",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/cores/esp32",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/variants/esp32s3",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src",
        "-I/home/sam/Arduino/libraries/PubSubClient/src",
        "-I/home/sam/Arduino/libraries/Freenove_WS2812_Lib_for_ESP32/src",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/build_opt.h",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/file_opts",
        "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src/WiFiGeneric.cpp",
        "-o",
        "/dev/null"
      ]
    }
  },
  {
    "missing_include_h": ""
  },
  {
    "compile": {
      "source_path": "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src/WiFiMulti.cpp",
      "object_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/WiFi/WiFiMulti.cpp.o",
      "depfile_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/WiFi/WiFiMulti.cpp.d"
    },
    "compile_task": {
      "args": [
        "/home/sam/.arduino15/packages/esp32/tools/esp-x32/2411/bin/xtensa-esp32s3-elf-g++",
        "-c",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/cpp_flags",
        "-w",
        "-Os",
        "-Werror=return-type",
        "-w",
        "-x",
        "c++",
        "-E",
        "-CC",
        "-DF_CPU=240000000L",
        "-DARDUINO=10607",
        "-DARDUINO_ESP32S3_DEV",
        "-DARDUINO_ARCH_ESP32",
        "-DARDUINO_BOARD=\"ESP32S3_DEV\"",
        "-DARDUINO_VARIANT=\"esp32s3\"",
        "-DARDUINO_PARTITION_default",
        "-DARDUINO_HOST_OS=\"linux\"",
        "-DARDUINO_FQBN=\"esp32:esp32:esp32s3:CDCOnBoot=cdc,USBMode=hwcdc,PSRAM=disabled,FlashMode=dio,DebugLevel=info\"",
        "-DESP32=ESP32",
        "-DCORE_DEBUG_LEVEL=3",
        "-DARDUINO_RUNNING_CORE=1",
        "-DARDUINO_EVENT_RUNNING_CORE=1",
        "-DARDUINO_USB_MODE=1",
        "-DARDUINO_USB_CDC_ON_BOOT=1",
        "-DARDUINO_USB_MSC_ON_BOOT=0",
        "-DARDUINO_USB_DFU_ON_BOOT=0",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/defines",
        "-I/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant",
        "-iprefix",
        "/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/include/",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/includes",
        "-I/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/dio_qspi/include",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/cores/esp32",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/variants/esp32s3",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src",
        "-I/home/sam/Arduino/libraries/PubSubClient/src",
        "-I/home/sam/Arduino/libraries/Freenove_WS2812_Lib_for_ESP32/src",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/build_opt.h",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/file_opts",
        "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src/WiFiMulti.cpp",
        "-o",
        "/dev/null"
      ]
    }
  },
  {
    "missing_include_h": ""
  },
  {
    "compile": {
      "source_path": "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src/WiFiSTA.cpp",
      "object_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/WiFi/WiFiSTA.cpp.o",
      "depfile_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/WiFi/WiFiSTA.cpp.d"
    },
    "compile_task": {
      "args": [
        "/home/sam/.arduino15/packages/esp32/tools/esp-x32/2411/bin/xtensa-esp32s3-elf-g++",
        "-c",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/cpp_flags",
        "-w",
        "-Os",
        "-Werror=return-type",
        "-w",
        "-x",
        "c++",
        "-E",
        "-CC",
        "-DF_CPU=240000000L",
        "-DARDUINO=10607",
        "-DARDUINO_ESP32S3_DEV",
        "-DARDUINO_ARCH_ESP32",
        "-DARDUINO_BOARD=\"ESP32S3_DEV\"",
        "-DARDUINO_VARIANT=\"esp32s3\"",
        "-DARDUINO_PARTITION_default",
        "-DARDUINO_HOST_OS=\"linux\"",
        "-DARDUINO_FQBN=\"esp32:esp32:esp32s3:CDCOnBoot=cdc,USBMode=hwcdc,PSRAM=disabled,FlashMode=dio,DebugLevel=info\"",
        "-DESP32=ESP32",
        "-DCORE_DEBUG_LEVEL=3",
        "-DARDUINO_RUNNING_CORE=1",
        "-DARDUINO_EVENT_RUNNING_CORE=1",
        "-DARDUINO_USB_MODE=1",
        "-DARDUINO_USB_CDC_ON_BOOT=1",
        "-DARDUINO_USB_MSC_ON_BOOT=0",
        "-DARDUINO_USB_DFU_ON_BOOT=0",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/defines",
        "-I/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant",
        "-iprefix",
        "/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/include/",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/includes",
        "-I/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/dio_qspi/include",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/cores/esp32",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/variants/esp32s3",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src",
        "-I/home/sam/Arduino/libraries/PubSubClient/src",
        "-I/home/sam/Arduino/libraries/Freenove_WS2812_Lib_for_ESP32/src",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/build_opt.h",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/file_opts",
        "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src/WiFiSTA.cpp",
        "-o",
        "/dev/null"
      ]
    }
  },
  {
    "missing_include_h": ""
  },
  {
    "compile": {
      "source_path": "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src/WiFiScan.cpp",
      "object_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/WiFi/WiFiScan.cpp.o",
      "depfile_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/WiFi/WiFiScan.cpp.d"
    },
    "compile_task": {
      "args": [
        "/home/sam/.arduino15/packages/esp32/tools/esp-x32/2411/bin/xtensa-esp32s3-elf-g++",
        "-c",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/cpp_flags",
        "-w",
        "-Os",
        "-Werror=return-type",
        "-w",
        "-x",
        "c++",
        "-E",
        "-CC",
        "-DF_CPU=240000000L",
        "-DARDUINO=10607",
        "-DARDUINO_ESP32S3_DEV",
        "-DARDUINO_ARCH_ESP32",
        "-DARDUINO_BOARD=\"ESP32S3_DEV\"",
        "-DARDUINO_VARIANT=\"esp32s3\"",
        "-DARDUINO_PARTITION_default",
        "-DARDUINO_HOST_OS=\"linux\"",
        "-DARDUINO_FQBN=\"esp32:esp32:esp32s3:CDCOnBoot=cdc,USBMode=hwcdc,PSRAM=disabled,FlashMode=dio,DebugLevel=info\"",
        "-DESP32=ESP32",
        "-DCORE_DEBUG_LEVEL=3",
        "-DARDUINO_RUNNING_CORE=1",
        "-DARDUINO_EVENT_RUNNING_CORE=1",
        "-DARDUINO_USB_MODE=1",
        "-DARDUINO_USB_CDC_ON_BOOT=1",
        "-DARDUINO_USB_MSC_ON_BOOT=0",
        "-DARDUINO_USB_DFU_ON_BOOT=0",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/defines",
        "-I/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant",
        "-iprefix",
        "/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/include/",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/includes",
        "-I/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/dio_qspi/include",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/cores/esp32",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/variants/esp32s3",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src",
        "-I/home/sam/Arduino/libraries/PubSubClient/src",
        "-I/home/sam/Arduino/libraries/Freenove_WS2812_Lib_for_ESP32/src",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/build_opt.h",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/file_opts",
        "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src/WiFiScan.cpp",
        "-o",
        "/dev/null"
      ]
    }
  },
  {
    "missing_include_h": ""
  },
  {
    "compile": {
      "source_path": "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src/NetworkClient.cpp",
      "object_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/Network/NetworkClient.cpp.o",
      "depfile_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/Network/NetworkClient.cpp.d"
    },
    "compile_task": {
      "args": [
        "/home/sam/.arduino15/packages/esp32/tools/esp-x32/2411/bin/xtensa-esp32s3-elf-g++",
        "-c",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/cpp_flags",
        "-w",
        "-Os",
        "-Werror=return-type",
        "-w",
        "-x",
        "c++",
        "-E",
        "-CC",
        "-DF_CPU=240000000L",
        "-DARDUINO=10607",
        "-DARDUINO_ESP32S3_DEV",
        "-DARDUINO_ARCH_ESP32",
        "-DARDUINO_BOARD=\"ESP32S3_DEV\"",
        "-DARDUINO_VARIANT=\"esp32s3\"",
        "-DARDUINO_PARTITION_default",
        "-DARDUINO_HOST_OS=\"linux\"",
        "-DARDUINO_FQBN=\"esp32:esp32:esp32s3:CDCOnBoot=cdc,USBMode=hwcdc,PSRAM=disabled,FlashMode=dio,DebugLevel=info\"",
        "-DESP32=ESP32",
        "-DCORE_DEBUG_LEVEL=3",
        "-DARDUINO_RUNNING_CORE=1",
        "-DARDUINO_EVENT_RUNNING_CORE=1",
        "-DARDUINO_USB_MODE=1",
        "-DARDUINO_USB_CDC_ON_BOOT=1",
        "-DARDUINO_USB_MSC_ON_BOOT=0",
        "-DARDUINO_USB_DFU_ON_BOOT=0",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/defines",
        "-I/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant",
        "-iprefix",
        "/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/include/",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/includes",
        "-I/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/dio_qspi/include",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/cores/esp32",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/variants/esp32s3",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src",
        "-I/home/sam/Arduino/libraries/PubSubClient/src",
        "-I/home/sam/Arduino/libraries/Freenove_WS2812_Lib_for_ESP32/src",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/build_opt.h",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/file_opts",
        "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src/NetworkClient.cpp",
        "-o",
        "/dev/null"
      ]
    }
  },
  {
    "missing_include_h": ""
  },
  {
    "compile": {
      "source_path": "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src/NetworkEvents.cpp",
      "object_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/Network/NetworkEvents.cpp.o",
      "depfile_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/Network/NetworkEvents.cpp.d"
    },
    "compile_task": {
      "args": [
        "/home/sam/.arduino15/packages/esp32/tools/esp-x32/2411/bin/xtensa-esp32s3-elf-g++",
        "-c",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/cpp_flags",
        "-w",
        "-Os",
        "-Werror=return-type",
        "-w",
        "-x",
        "c++",
        "-E",
        "-CC",
        "-DF_CPU=240000000L",
        "-DARDUINO=10607",
        "-DARDUINO_ESP32S3_DEV",
        "-DARDUINO_ARCH_ESP32",
        "-DARDUINO_BOARD=\"ESP32S3_DEV\"",
        "-DARDUINO_VARIANT=\"esp32s3\"",
        "-DARDUINO_PARTITION_default",
        "-DARDUINO_HOST_OS=\"linux\"",
        "-DARDUINO_FQBN=\"esp32:esp32:esp32s3:CDCOnBoot=cdc,USBMode=hwcdc,PSRAM=disabled,FlashMode=dio,DebugLevel=info\"",
        "-DESP32=ESP32",
        "-DCORE_DEBUG_LEVEL=3",
        "-DARDUINO_RUNNING_CORE=1",
        "-DARDUINO_EVENT_RUNNING_CORE=1",
        "-DARDUINO_USB_MODE=1",
        "-DARDUINO_USB_CDC_ON_BOOT=1",
        "-DARDUINO_USB_MSC_ON_BOOT=0",
        "-DARDUINO_USB_DFU_ON_BOOT=0",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/defines",
        "-I/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant",
        "-iprefix",
        "/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/include/",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/includes",
        "-I/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/dio_qspi/include",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/cores/esp32",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/variants/esp32s3",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src",
        "-I/home/sam/Arduino/libraries/PubSubClient/src",
        "-I/home/sam/Arduino/libraries/Freenove_WS2812_Lib_for_ESP32/src",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/build_opt.h",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/file_opts",
        "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src/NetworkEvents.cpp",
        "-o",
        "/dev/null"
      ]
    }
  },
  {
    "missing_include_h": ""
  },
  {
    "compile": {
      "source_path": "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src/NetworkInterface.cpp",
      "object_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/Network/NetworkInterface.cpp.o",
      "depfile_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/Network/NetworkInterface.cpp.d"
    },
    "compile_task": {
      "args": [
        "/home/sam/.arduino15/packages/esp32/tools/esp-x32/2411/bin/xtensa-esp32s3-elf-g++",
        "-c",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/cpp_flags",
        "-w",
        "-Os",
        "-Werror=return-type",
        "-w",
        "-x",
        "c++",
        "-E",
        "-CC",
        "-DF_CPU=240000000L",
        "-DARDUINO=10607",
        "-DARDUINO_ESP32S3_DEV",
        "-DARDUINO_ARCH_ESP32",
        "-DARDUINO_BOARD=\"ESP32S3_DEV\"",
        "-DARDUINO_VARIANT=\"esp32s3\"",
        "-DARDUINO_PARTITION_default",
        "-DARDUINO_HOST_OS=\"linux\"",
        "-DARDUINO_FQBN=\"esp32:esp32:esp32s3:CDCOnBoot=cdc,USBMode=hwcdc,PSRAM=disabled,FlashMode=dio,DebugLevel=info\"",
        "-DESP32=ESP32",
        "-DCORE_DEBUG_LEVEL=3",
        "-DARDUINO_RUNNING_CORE=1",
        "-DARDUINO_EVENT_RUNNING_CORE=1",
        "-DARDUINO_USB_MODE=1",
        "-DARDUINO_USB_CDC_ON_BOOT=1",
        "-DARDUINO_USB_MSC_ON_BOOT=0",
        "-DARDUINO_USB_DFU_ON_BOOT=0",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/defines",
        "-I/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant",
        "-iprefix",
        "/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/include/",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/includes",
        "-I/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/dio_qspi/include",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/cores/esp32",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/variants/esp32s3",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src",
        "-I/home/sam/Arduino/libraries/PubSubClient/src",
        "-I/home/sam/Arduino/libraries/Freenove_WS2812_Lib_for_ESP32/src",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/build_opt.h",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/file_opts",
        "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src/NetworkInterface.cpp",
        "-o",
        "/dev/null"
      ]
    }
  },
  {
    "missing_include_h": ""
  },
  {
    "compile": {
      "source_path": "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src/NetworkManager.cpp",
      "object_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/Network/NetworkManager.cpp.o",
      "depfile_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/Network/NetworkManager.cpp.d"
    },
    "compile_task": {
      "args": [
        "/home/sam/.arduino15/packages/esp32/tools/esp-x32/2411/bin/xtensa-esp32s3-elf-g++",
        "-c",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/cpp_flags",
        "-w",
        "-Os",
        "-Werror=return-type",
        "-w",
        "-x",
        "c++",
        "-E",
        "-CC",
        "-DF_CPU=240000000L",
        "-DARDUINO=10607",
        "-DARDUINO_ESP32S3_DEV",
        "-DARDUINO_ARCH_ESP32",
        "-DARDUINO_BOARD=\"ESP32S3_DEV\"",
        "-DARDUINO_VARIANT=\"esp32s3\"",
        "-DARDUINO_PARTITION_default",
        "-DARDUINO_HOST_OS=\"linux\"",
        "-DARDUINO_FQBN=\"esp32:esp32:esp32s3:CDCOnBoot=cdc,USBMode=hwcdc,PSRAM=disabled,FlashMode=dio,DebugLevel=info\"",
        "-DESP32=ESP32",
        "-DCORE_DEBUG_LEVEL=3",
        "-DARDUINO_RUNNING_CORE=1",
        "-DARDUINO_EVENT_RUNNING_CORE=1",
        "-DARDUINO_USB_MODE=1",
        "-DARDUINO_USB_CDC_ON_BOOT=1",
        "-DARDUINO_USB_MSC_ON_BOOT=0",
        "-DARDUINO_USB_DFU_ON_BOOT=0",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/defines",
        "-I/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant",
        "-iprefix",
        "/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/include/",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/includes",
        "-I/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/dio_qspi/include",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/cores/esp32",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/variants/esp32s3",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src",
        "-I/home/sam/Arduino/libraries/PubSubClient/src",
        "-I/home/sam/Arduino/libraries/Freenove_WS2812_Lib_for_ESP32/src",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/build_opt.h",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/file_opts",
        "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src/NetworkManager.cpp",
        "-o",
        "/dev/null"
      ]
    }
  },
  {
    "missing_include_h": ""
  },
  {
    "compile": {
      "source_path": "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src/NetworkServer.cpp",
      "object_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/Network/NetworkServer.cpp.o",
      "depfile_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/Network/NetworkServer.cpp.d"
    },
    "compile_task": {
      "args": [
        "/home/sam/.arduino15/packages/esp32/tools/esp-x32/2411/bin/xtensa-esp32s3-elf-g++",
        "-c",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/cpp_flags",
        "-w",
        "-Os",
        "-Werror=return-type",
        "-w",
        "-x",
        "c++",
        "-E",
        "-CC",
        "-DF_CPU=240000000L",
        "-DARDUINO=10607",
        "-DARDUINO_ESP32S3_DEV",
        "-DARDUINO_ARCH_ESP32",
        "-DARDUINO_BOARD=\"ESP32S3_DEV\"",
        "-DARDUINO_VARIANT=\"esp32s3\"",
        "-DARDUINO_PARTITION_default",
        "-DARDUINO_HOST_OS=\"linux\"",
        "-DARDUINO_FQBN=\"esp32:esp32:esp32s3:CDCOnBoot=cdc,USBMode=hwcdc,PSRAM=disabled,FlashMode=dio,DebugLevel=info\"",
        "-DESP32=ESP32",
        "-DCORE_DEBUG_LEVEL=3",
        "-DARDUINO_RUNNING_CORE=1",
        "-DARDUINO_EVENT_RUNNING_CORE=1",
        "-DARDUINO_USB_MODE=1",
        "-DARDUINO_USB_CDC_ON_BOOT=1",
        "-DARDUINO_USB_MSC_ON_BOOT=0",
        "-DARDUINO_USB_DFU_ON_BOOT=0",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/defines",
        "-I/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant",
        "-iprefix",
        "/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/include/",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/includes",
        "-I/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/dio_qspi/include",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/cores/esp32",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/variants/esp32s3",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src",
        "-I/home/sam/Arduino/libraries/PubSubClient/src",
        "-I/home/sam/Arduino/libraries/Freenove_WS2812_Lib_for_ESP32/src",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/build_opt.h",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/file_opts",
        "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src/NetworkServer.cpp",
        "-o",
        "/dev/null"
      ]
    }
  },
  {
    "missing_include_h": ""
  },
  {
    "compile": {
      "source_path": "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src/NetworkUdp.cpp",
      "object_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/Network/NetworkUdp.cpp.o",
      "depfile_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/Network/NetworkUdp.cpp.d"
    },
    "compile_task": {
      "args": [
        "/home/sam/.arduino15/packages/esp32/tools/esp-x32/2411/bin/xtensa-esp32s3-elf-g++",
        "-c",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/cpp_flags",
        "-w",
        "-Os",
        "-Werror=return-type",
        "-w",
        "-x",
        "c++",
        "-E",
        "-CC",
        "-DF_CPU=240000000L",
        "-DARDUINO=10607",
        "-DARDUINO_ESP32S3_DEV",
        "-DARDUINO_ARCH_ESP32",
        "-DARDUINO_BOARD=\"ESP32S3_DEV\"",
        "-DARDUINO_VARIANT=\"esp32s3\"",
        "-DARDUINO_PARTITION_default",
        "-DARDUINO_HOST_OS=\"linux\"",
        "-DARDUINO_FQBN=\"esp32:esp32:esp32s3:CDCOnBoot=cdc,USBMode=hwcdc,PSRAM=disabled,FlashMode=dio,DebugLevel=info\"",
        "-DESP32=ESP32",
        "-DCORE_DEBUG_LEVEL=3",
        "-DARDUINO_RUNNING_CORE=1",
        "-DARDUINO_EVENT_RUNNING_CORE=1",
        "-DARDUINO_USB_MODE=1",
        "-DARDUINO_USB_CDC_ON_BOOT=1",
        "-DARDUINO_USB_MSC_ON_BOOT=0",
        "-DARDUINO_USB_DFU_ON_BOOT=0",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/defines",
        "-I/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant",
        "-iprefix",
        "/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/include/",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/includes",
        "-I/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/dio_qspi/include",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/cores/esp32",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/variants/esp32s3",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src",
        "-I/home/sam/Arduino/libraries/PubSubClient/src",
        "-I/home/sam/Arduino/libraries/Freenove_WS2812_Lib_for_ESP32/src",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/build_opt.h",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/file_opts",
        "/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src/NetworkUdp.cpp",
        "-o",
        "/dev/null"
      ]
    }
  },
  {
    "missing_include_h": ""
  },
  {
    "compile": {
      "source_path": "/home/sam/Arduino/libraries/PubSubClient/src/PubSubClient.cpp",
      "object_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/PubSubClient/PubSubClient.cpp.o",
      "depfile_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/PubSubClient/PubSubClient.cpp.d"
    },
    "compile_task": {
      "args": [
        "/home/sam/.arduino15/packages/esp32/tools/esp-x32/2411/bin/xtensa-esp32s3-elf-g++",
        "-c",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/cpp_flags",
        "-w",
        "-Os",
        "-Werror=return-type",
        "-w",
        "-x",
        "c++",
        "-E",
        "-CC",
        "-DF_CPU=240000000L",
        "-DARDUINO=10607",
        "-DARDUINO_ESP32S3_DEV",
        "-DARDUINO_ARCH_ESP32",
        "-DARDUINO_BOARD=\"ESP32S3_DEV\"",
        "-DARDUINO_VARIANT=\"esp32s3\"",
        "-DARDUINO_PARTITION_default",
        "-DARDUINO_HOST_OS=\"linux\"",
        "-DARDUINO_FQBN=\"esp32:esp32:esp32s3:CDCOnBoot=cdc,USBMode=hwcdc,PSRAM=disabled,FlashMode=dio,DebugLevel=info\"",
        "-DESP32=ESP32",
        "-DCORE_DEBUG_LEVEL=3",
        "-DARDUINO_RUNNING_CORE=1",
        "-DARDUINO_EVENT_RUNNING_CORE=1",
        "-DARDUINO_USB_MODE=1",
        "-DARDUINO_USB_CDC_ON_BOOT=1",
        "-DARDUINO_USB_MSC_ON_BOOT=0",
        "-DARDUINO_USB_DFU_ON_BOOT=0",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/defines",
        "-I/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant",
        "-iprefix",
        "/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/include/",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/includes",
        "-I/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/dio_qspi/include",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/cores/esp32",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/variants/esp32s3",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src",
        "-I/home/sam/Arduino/libraries/PubSubClient/src",
        "-I/home/sam/Arduino/libraries/Freenove_WS2812_Lib_for_ESP32/src",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/build_opt.h",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/file_opts",
        "/home/sam/Arduino/libraries/PubSubClient/src/PubSubClient.cpp",
        "-o",
        "/dev/null"
      ]
    }
  },
  {
    "missing_include_h": ""
  },
  {
    "compile": {
      "source_path": "/home/sam/Arduino/libraries/Freenove_WS2812_Lib_for_ESP32/src/Freenove_WS2812_Lib_for_ESP32.cpp",
      "object_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/Freenove_WS2812_Lib_for_ESP32/Freenove_WS2812_Lib_for_ESP32.cpp.o",
      "depfile_path": "/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/libraries/Freenove_WS2812_Lib_for_ESP32/Freenove_WS2812_Lib_for_ESP32.cpp.d"
    },
    "compile_task": {
      "args": [
        "/home/sam/.arduino15/packages/esp32/tools/esp-x32/2411/bin/xtensa-esp32s3-elf-g++",
        "-c",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/cpp_flags",
        "-w",
        "-Os",
        "-Werror=return-type",
        "-w",
        "-x",
        "c++",
        "-E",
        "-CC",
        "-DF_CPU=240000000L",
        "-DARDUINO=10607",
        "-DARDUINO_ESP32S3_DEV",
        "-DARDUINO_ARCH_ESP32",
        "-DARDUINO_BOARD=\"ESP32S3_DEV\"",
        "-DARDUINO_VARIANT=\"esp32s3\"",
        "-DARDUINO_PARTITION_default",
        "-DARDUINO_HOST_OS=\"linux\"",
        "-DARDUINO_FQBN=\"esp32:esp32:esp32s3:CDCOnBoot=cdc,USBMode=hwcdc,PSRAM=disabled,FlashMode=dio,DebugLevel=info\"",
        "-DESP32=ESP32",
        "-DCORE_DEBUG_LEVEL=3",
        "-DARDUINO_RUNNING_CORE=1",
        "-DARDUINO_EVENT_RUNNING_CORE=1",
        "-DARDUINO_USB_MODE=1",
        "-DARDUINO_USB_CDC_ON_BOOT=1",
        "-DARDUINO_USB_MSC_ON_BOOT=0",
        "-DARDUINO_USB_DFU_ON_BOOT=0",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/defines",
        "-I/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant",
        "-iprefix",
        "/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/include/",
        "@/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/flags/includes",
        "-I/home/sam/.arduino15/packages/esp32/tools/esp32-arduino-libs/idf-release_v5.5-129cd0d2-v4/esp32s3/dio_qspi/include",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/cores/esp32",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/variants/esp32s3",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/WiFi/src",
        "-I/home/sam/.arduino15/packages/esp32/hardware/esp32/3.3.1/libraries/Network/src",
        "-I/home/sam/Arduino/libraries/PubSubClient/src",
        "-I/home/sam/Arduino/libraries/Freenove_WS2812_Lib_for_ESP32/src",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/build_opt.h",
        "@/media/sam/8294CD2994CD2111/Users/Dell/Documents/Arduino/voice_assistant/build/file_opts",
        "/home/sam/Arduino/libraries/Freenove_WS2812_Lib_for_ESP32/src/Freenove_WS2812_Lib_for_ESP32.cpp",
        "-o",
        "/dev/null"
      ]
    }
  },
  {
    "missing_include_h": ""
  }
]